S-1233.1

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**SUBSTITUTE SENATE BILL 5282**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**State of Washington 64th Legislature 2015 Regular Session**

**By** Senate Commerce & Labor (originally sponsored by Senators Braun, Baumgartner, and Warnick)

AN ACT Relating to residential security system installations; and amending RCW 19.28.006 and 19.28.261.

BE IT ENACTED BY THE LEGISLATURE OF THE STATE OF WASHINGTON:

**Sec.**  RCW 19.28.006 and 2013 c 23 s 27 are each amended to read as follows:

The definitions in this section apply throughout this subchapter.

(1) "Administrator" means a person designated by an electrical contractor to supervise electrical work and electricians in accordance with the rules adopted under this chapter.

(2) "Basic electrical work" means the work classified in (a) and (b) of this subsection as class A and class B basic electrical work:

(a) "Class A basic electrical work" means:

(i) The like-in-kind replacement of a: Contactor, relay, timer, starter, circuit board, or similar control component; household appliance; circuit breaker; fuse; residential luminaire; lamp; snap switch; dimmer; receptacle outlet; thermostat; heating element; luminaire ballast with an exact same ballast; ten horsepower or smaller motor; or wiring, appliances, devices, or equipment as specified by rule.

(ii) Work limited to installing in a one or two family dwelling no more than one power supply cable six feet or less in length from a listed class two transformer rated no greater than twenty-four volts in connection with the installation, repair, or maintenance of one main control panel for a low voltage security, intrusion, or similar alarm system, excluding systems that monitor required fire or smoke detection devices.

(b) "Class B basic electrical work" means work other than class A basic electrical work that requires minimal electrical circuit modifications and has limited exposure hazards. Class B basic electrical work includes the following:

(i) Extension of not more than one branch electrical circuit limited to one hundred twenty volts and twenty amps each where:

(A) No cover inspection is necessary; and

(B) The extension does not supply more than two outlets;

(ii) Like-in-kind replacement of a single luminaire not exceeding two hundred seventy-seven volts and twenty amps;

(iii) Like-in-kind replacement of a motor larger than ten horsepower;

(iv) The following low voltage systems:

(A) Repair and replacement of devices not exceeding one hundred volt-amperes in Class 2, Class 3, or power limited low voltage systems in one and two-family dwellings;

(B) Repair and replacement of the following devices not exceeding one hundred volt-amperes in Class 2, Class 3, or power limited low voltage systems in other buildings, provided the equipment is not for fire alarm or nurse call systems and is not located in an area classified as hazardous by the national electrical code; or

(v) Wiring, appliances, devices, or equipment as specified by rule.

(3) "Board" means the electrical board under RCW 19.28.311.

(4) "Chapter" or "subchapter" means the subchapter, if no chapter number is referenced.

(5) "Department" means the department of labor and industries.

(6) "Director" means the director of the department or the director's designee.

(7) "Electrical construction trade" includes, but is not limited to, installing or maintaining electrical wires and equipment that are used for light, heat, or power and installing and maintaining remote control, signaling, power limited, or communication circuits or systems.

(8) "Electrical contractor" means a person, firm, partnership, corporation, or other entity that offers to undertake, undertakes, submits a bid for, or does the work of installing or maintaining wires or equipment that convey electrical current.

(9) "Equipment" means any equipment or apparatus that directly uses, conducts, insulates, or is operated by electricity but does not mean: Plug-in appliances; or plug-in equipment as determined by the department by rule.

(10) "Industrial control panel" means a factory-wired or user-wired assembly of industrial control equipment such as motor controllers, switches, relays, power supplies, computers, cathode ray tubes, transducers, and auxiliary devices. The panel may include disconnect means and motor branch circuit protective devices.

(11) "Journey level electrician" means a person who has been issued a journey level electrician certificate of competency by the department.

(12) "Like-in-kind" means having similar characteristics such as voltage requirements, current draw, and function, and being in the same location.

(13) "Master electrician" means either a master journey level electrician or master specialty electrician.

(14) "Master journey level electrician" means a person who has been issued a master journey level electrician certificate of competency by the department and who may be designated by an electrical contractor to supervise electrical work and electricians in accordance with rules adopted under this chapter.

(15) "Master specialty electrician" means a person who has been issued a specialty electrician certificate of competency by the department and who may be designated by an electrical contractor to supervise electrical work and electricians in accordance with rules adopted under this chapter.

(16) "Specialty electrician" means a person who has been issued a specialty electrician certificate of competency by the department.

**Sec.**  RCW 19.28.261 and 2013 c 23 s 37 are each amended to read as follows:

(1) Nothing in RCW 19.28.161 through 19.28.271 shall be construed to require that a person obtain a license or a certified electrician in order to do electrical work at his or her residence or farm or place of business or on other property owned by him or her unless the electrical work is on the construction of a new building intended for rent, sale, or lease. However, if the construction is of a new residential building with up to four units intended for rent, sale, or lease, the owner may receive an exemption from the requirement to obtain a license or use a certified electrician if he or she provides a signed affidavit to the department stating that he or she will be performing the work and will occupy one of the units as his or her principal residence. The owner shall apply to the department for this exemption and may only receive an exemption once every twenty-four months. It is intended that the owner receiving this exemption shall occupy the unit as his or her principal residence for twenty-four months after completion of the units.

(2) Nothing in RCW 19.28.161 through 19.28.271 shall be intended to derogate from or dispense with the requirements of any valid electrical code enacted by a city or town pursuant to RCW 19.28.010(3), except that no code shall require the holder of a certificate of competency to demonstrate any additional proof of competency or obtain any other license or pay any fee in order to engage in the electrical construction trade.

(3) RCW 19.28.161 through 19.28.271 shall not apply to common carriers subject to Part I of the Interstate Commerce Act, nor to their officers and employees.

(4) Nothing in RCW 19.28.161 through 19.28.271 shall be deemed to apply to the installation or maintenance of telephone, telegraph, radio, or television wires and equipment; nor to any electrical utility or its employees in the installation, repair, and maintenance of electrical wiring, circuits, and equipment by or for the utility, or comprising a part of its plants, lines, or systems.

(5) The licensing provisions of RCW 19.28.161 through 19.28.271 shall not apply to:

(a) Persons making electrical installations on their own property or to regularly employed employees working on the premises of their employer, unless the electrical work is on the construction of a new building intended for rent, sale, or lease;

(b) Employees of an employer while the employer is performing utility type work of the nature described in RCW 19.28.091 so long as such employees have registered in the state of Washington with or graduated from a state-approved outside lineworker apprenticeship course that is recognized by the department and that qualifies a person to perform such work;

(c) Any work exempted under RCW 19.28.091(6); and

(d) Certified plumbers, certified residential plumbers, or plumber trainees meeting the requirements of chapter 18.106 RCW and performing exempt work under RCW 19.28.091(8).

(6) Nothing in RCW 19.28.161 through 19.28.271 shall be construed to restrict the right of any householder to assist or receive assistance from a friend, neighbor, relative, or other person when none of the individuals doing the electrical installation hold themselves out as engaged in the trade or business of electrical installations.

(7) Nothing precludes any person who is exempt from the licensing requirements of this chapter under this section from obtaining a journey level or specialty certificate of competency if they otherwise meet the requirements of this chapter.

(8) RCW 19.28.161 through 19.28.271 shall not apply to persons performing work limited to installing in a one or two family dwelling no more than one power supply cable six feet or less in length from a listed class two transformer rated no greater than twenty-four volts in connection with the installation, repair, or maintenance of one main control panel for a low voltage security, intrusion, or similar alarm system, excluding systems that monitor required fire or smoke detection devices.

**--- END ---**